# Greco V2 Quick Test Cuff

This is an optional short-print sample before committing to the full Greco V2 planter. It uses the actual v2 radii over the flute and Greek-key band zone.

## What to print first if you want a risk check

1. Download greco-planter-v2-quick-cuff.stl.
2. Reslice it for your own printer/material/profile. This quick cuff package does not include printer-ready G-code.
3. If the Greek-key band fuses, flutes look rough, or the wall feels weak, tune settings before starting the full 120 mm planter.

## Sample facts

Print candidate | `greco-planter-v2-quick-cuff.stl`
Source geometry | Actual Greco V2 outer and inner radii, full circumference
Source z range | 66.0–101.5 mm from the full planter
Printed height | 35.5 mm
Outer footprint | about 93.6 x 93.6 mm
Minimum radial wall | about 3.8 mm in the flute trough zone
Purpose | Tests the thinnest flute wall, band rails, and Greek-key/meander relief without committing to the full print.

## Caveats

- No physical print was performed for this quick cuff.
- The cuff is a printer/material risk sample, not a substitute for the full planter body, rim, base, or drain test.
- Reslice the STL before print. Estimates vary by printer, material, and slicer profile.
- Watertight mesh means valid geometry, not a sealed vessel claim.