Greco V2 Quick Test Cuff handoff
Generated: 2026-06-23T11:31:20.418252+00:00

Files:
- greco-planter-v2-quick-cuff-guide.html — public guide and caveats.
- greco-planter-v2-quick-cuff.stl — quick-print cuff STL using actual v2 radii.
- evidence/greco-planter-v2-quick-cuff-surface-sheet.jpg — all-angle surface preview.
- report/greco-planter-v2-quick-cuff-report.json — sanitized mesh/geometry report.

Geometry:
- Source z range: 66.0–101.5 mm from the full planter.
- Printed height: 35.5 mm.
- Footprint: 93.5 x 93.6 mm.
- Minimum radial wall: 3.80 mm.

Caveats:
- No physical print was performed.
- This package contains no printer-ready G-code. Reslice the STL.
- The cuff tests flute/meander wall quality before the full print; it is not the full planter.
